Årtull

Nutisk Ordbok - 1914

Tullpinne {Thole pin, thole) [Dolle, Bootsdolle] är egentligen en i relingen nedsatt pinne af hårdt trä, hvaremot åran stöder under rodd, såsom på de flesta allmogebåtar, men ordet begagnas äfven för att beteckna andra inrättningar till stöd för åran. Tullbord {thole stringer) [Kojenleiste], en förstärkning långs med relingen till stöd för tullpinnarne.

Svenskt Nautiskt Lexikon - 1920

Tollpinnar, tullar eller årtullar, pinnar av trä eller järn, som stickas i hål i relingen på en båt att lägga årorna emellan vid rodd. På tullbordet finnes ofta emellan tullarna en roddlapp för årån att slita på.

The Sailor's Word-Book - 1867

THOLE, THOLE-PIN, OR THOWEL [from the Anglo-Saxon thol]. Certain pins in the
gunwale of a boat, instead of the rowlock-poppets, and serving to retain the oars in
position when pulling; generally there is only one pin to each oar, which is retained upon
the pin by a grommet, or a cleat with a hole through it, nailed on the side of the oar. The
principal use is to allow the oar, in case of action, suddenly to lie fore-and-aft over the
side, and take care of itself. This was superseded by the swinging thowel, or metal
crutch, in 1819, and by admiralty order at Portsmouth Yard in 1830.

Dictionary of Nautical Words and Terms - 1982

Thole, Thole Pin. Metal or wooden peg inserted in gunwale of a boat for oar to heave against when rowing without crutch or rowlock.